1.CHECK POWER WINDOW SUB-SWITCH

1. Turn ignition switch OFF.
2. Disconnect power window sub-switch connector.
3. Check continuity between power window sub-switch terminals.

Power window sub-switch | Condition | Continuity
Connector | Terminal
D38 | 14 | 3 | AUTO | Existed
5 | Not existed
3 | Other than above | Not existed
5 | Existed
15 | 3 | UP | Existed
6 | Not existed
3 | Other than above | Not existed
6 | Existed
16 | 3 | DOWN | Existed
7 | Not existed
3 | Other than above | Not existed
7 | Existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace power window sub-switch. Refer to Removal and Installation.