INSPECTION Check valve Inspection Check that air can pass through the hose by blowing forward (toward the nozzle), and check that air cannot pass through by sucking. ADJUSTMENT Front Washer Nozzle Spray Position Adjustment
Adjust spray positions to match the positions shown in the figure. Remove the wiper motor connector to ensure front wiper arms do not move.

1. | Front washer nozzle | 2. | Passenger side blade rubber end | 3. | Driver side blade rubber end
| : Spray area |  |  |  |
| : Target spray position |  |  |  |

Unit: mm (in)
Spray position | T | L | X | Y | S
A | 29 (1.14) | 448 (17.64) | 20 (0.79) | 50 (1.97) | 25 (0.98)
B | 34 (1.34) | 235 (9.25) | 20 (0.79) | 20 (0.79) | 10 (0.39)
C | −18 (−0.71) | 112 (4.41) | 20 (0.79) | 20 (0.79) | 10 (0.39)
D | 29 (1.14) | 115 (4.53) | 20 (0.79) | 20 (0.79) | 10 (0.39)
E | 30 (1.18) | 304 (11.97) | 20 (0.79) | 30 (1.18) | 15 (0.59)
F | −40 (−1.57) | 237 (9.33) | 20 (0.79) | 60 (2.36) | 30 (1.18)
G | 35 (1.38) | 197 (7.76) | 20 (0.79) | 30 (1.18) | 15 (0.59)
H | 30 (1.18) | 73 (2.87) | 20 (0.79) | 20 (0.79) | 10 (0.39)
I | −17 (−0.67) | 68 (2.68) | 20 (0.79) | 20 (0.79) | 10 (0.39)

Insert a needle or similar object (A) into the spray opening (1) and move up/down and left/right to adjust the spray position.
NOTE：
If wax or dust gets into the nozzle, remove wax or dust with a needle or small pin.