REMOVAL ■ CAUTION ■ Never drop or strike rear vertical G sensor, or do not use power tool etc., because rear vertical G sensor is sensitive to the impact.

1.Turn the ignition switch OFF.

2.Remove the trunk side finisher lower LH. Refer to Exploded View.

3.Disconnect the rear vertical G sensor connector.

4.Remove the rear vertical G sensor mounting bolts.

5.Remove the rear vertical G sensor.

INSTALLATION
Installation is the reverse order of removal.
■ CAUTION ■
Never drop or strike rear vertical G sensor, or do not use power tool etc., because rear vertical G sensor is sensitive to the impact.