1.CHECK BRAKE FLUID LEVEL SWITCH

1. Turn the ignition switch OFF.
2. Disconnect brake fluid level switch harness connector.
3. Check the continuity between brake fluid level switch harness connector terminals.

   Brake fluid level switch | Condition | Continuity
   Terminal
   1 − 2 | When brake fluid is full in the reservoir tank. | Not existed
   When brake fluid is empty in the reservoir tank. | Existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace reservoir tank. Refer to Exploded View (GT-R certified NISSAN dealer).