1.CHECK ASCD BRAKE SWITCH-I

1. Turn ignition switch OFF.
2. Disconnect ASCD brake switch harness connector.
3. Check the continuity between ASCD brake switch terminals under the following conditions.

   Terminals | Condition | Continuity
   1 and 2 | Brake pedal | Fully released | Existed
   Slightly depressed | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>GO TO 2.
2.CHECK ASCD BRAKE SWITCH-II

1. Adjust ASCD brake switch installation. Refer to Inspection and Adjustment.
2. Check the continuity between ASCD brake switch terminals under the following conditions.

   Terminals | Condition | Continuity
   1 and 2 | Brake pedal | Fully released | Existed
   Slightly depressed | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace ASCD brake switch.