REMOVAL

1.Disconnect battery cable from negative terminal.

2.Remove the front diffuser. Refer to Exploded View.

3.Drain the transmission oil from the transmission assembly. Refer to Draining.

4.Disconnect the park position switch connector (A).

5.Remove the park position switch (1).

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Never reuse plain washer.
- Securely remove dust on screws.
- Never use gasket fluid or thread locking agent to threads.

- Install the park position switch with the parking lever in the P range (A).

  B | : Other than the P position

- Fill with the transmission oil to the transmission assembly after installation. Refer to Filling.