BCM CONSULT-III FUNCTION CONSULT-III performs the following functions via CAN communication with BCM.

Diagnosis mode | Function Description
WORK SUPPORT | Changes the setting for each system function.
DATA MONITOR | The BCM input/output signals are displayed.
ACTIVE TEST | The signals used to activate each device are forcibly supplied from BCM.

WORK SUPPORT

Monitor item | Description
DOOR LOCK-UNLOCK SET | Selective unlock function mode can be changed to operate (WITH) or not operate (WITHOUT) with this mode.
AUTOMATIC DOOR LOOK SELECT | Automatic door lock function mode can be selected from the following in this mode.

- VH SPD: All doors are locked when vehicle speed more than 24km/h(15MPH)
- P RANGE: All doors are locked when shifting the shift lever from P position to other than the P position

AUTOMATIC DOOR UNLOCK SELECT | Automatic door unlock function mode can be selected from the following in the mode.

- MODE 1: All doors are unlocked when the power supply position is changed from ON to OFF
- MODE 2: All doors are unlocked when shifting the shift lever from any position other than the P to P position
- MODE 3: Driver side door is unlocked when the power supply position is changed from ON to OFF
- MODE 4: Driver side door is unlocked when shifting the shift lever from any position other than the P to P position

AUTOMATIC LOCK/UNLOCK SET | Automatic door lock/unlock function mode can be selected from the following in this mode.

- Off: non-operational
- Unlock only: door unlock operation only
- Lock only: door lock operation only
- Lock/unlock: lock/unlock operation

DATA MONITOR

Monitor Item | Contents
REQ SW-DR | Indicated [ON/OFF] condition of door request switch (driver side).
REQ SW-AS | Indicated [ON/OFF] condition of door request switch (passenger side).
REQ SW-BD/TR | Indicated [ON/OFF] condition of trunk lid opener request switch.
DOOR SW-DR | Indicated [ON/OFF] condition of front door switch (driver side).
DOOR SW-AS | Indicated [ON/OFF] condition of front door switch (passenger side).
DOOR SW-RR | NOTE： This item is displayed, but cannot be monitored.
DOOR SW-RL | NOTE： This item is displayed, but cannot be monitored.
DOOR SW-BK | NOTE： This item is displayed, but cannot be monitored.
CDL LOCK SW | Indicated [ON/OFF] condition of lock signal from door lock unlock switch.
CDL UNLOCK SW | Indicated [ON/OFF] condition of unlock signal from door lock unlock switch.
KEY CYL LK-SW | NOTE： This item is displayed, but cannot be monitored.
KEY CYL UN-SW | NOTE： This item is displayed, but cannot be monitored.

ACTIVE TEST

Test item | Description
DOOR LOCK | This test is able to check door lock/unlock operation.

- The all door lock actuators are locked when “ALL LCK” on CONSULT-III screen is touched.
- The all door lock actuators are unlocked when “ALL UNLK” on CONSULT-III screen is touched.
- The door lock actuator (driver side) is unlocked when “DR UNLK” on CONSULT-III screen is touched.
- The door lock actuator (passenger side) is unlocked when “AS UNLK” on CONSULT- III screen is touched.
- “OTR ULK” item is displayed, but cannot be monitored.