REMOVAL

1.Disconnect the battery cable from the negative terminal.

2.Remove drive belt. Refer to Removal and Installation (GT-R certified NISSAN dealer).

3.Remove drive belt auto tensioner and idler pulley bracket side. Refer to Exploded View.

4.Remove engine front undercover, using power tools.

5.Remove alternator mounting upper bolt.

6.Disconnect oil pressure switch connector.

7.Pull up alternator, and then disconnect alternator connector (1).

8.Remove “B” terminal nut (2).

9.Remove alternator assembly upward from the vehicle.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■
Be sure to tighten “B” terminal nut carefully.
Install alternator, and check tension of belt. Refer to Checking.