1.PERFORM COMPONENT FUNCTION CHECK

1. Turn ignition switch ON.
2. Check the voltage between ECM harness connector terminals under the following conditions.

   ECM | Condition | Voltage (V)
   Connector | + | –
   Terminal | Terminal
   M107 | 111 | 128 | Selector lever | P or N | Battery voltage
   Except above | Approx. 0

Is the inspection result normal?
YES>>INSPECTION END
NO>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).