BCM CONSULT-III FUNCTION CONSULT-III performs the following functions via CAN communication with BCM.

Diagnosis mode | Function Description
WORK SUPPORT | Changes the setting for each system function.
SELF-DIAG RESULTS | Displays the diagnosis results judged by BCM.
DATA MONITOR | The BCM input/output signals are displayed.
ACTIVE TEST | The signals used to activate each device are forcibly supplied from BCM.

WORK SUPPORT

Monitor item | Description
REMO CONT ID CONFIR | It can be checked whether Intelligent Key ID code is registered or not in this mode.
AUTO LOCK SET | Auto door lock time can be changed in this mode.

- MODE 1: 1 minute
- MODE 2: 5 minutes
- MODE 3: 30 seconds
- MODE 4: 2 minutes

LOCK/UNLOCK BY I-KEY | Door lock/unlock function by door request switch (driver side and passenger side) mode can be changed to operate (WITH) or not operate (WITHOUT) in this mode.
ENGINE START BY I-KEY | Engine start function mode can be changed to operate (WITH) or not operate (WITHOUT) in this mode.
TRUNK/GLASS HATCH OPEN | Buzzer reminder function mode by trunk lid opener request switch can be changed to operate (WITH) or not operate (WITHOUT) in this mode.
PANIC ALARM SET | Panic alarm button pressing time on Intelligent Key remote control button can be selected from the following wit this mode.

- MODE 1: 0.5 sec.
- MODE 2: OFF: Non-operation
- MODE 3: 1.5 sec.

PW DOWN SET | This item is displayed, but cannot be used.
TRUNK OPEN DELAY | Trunk button pressing on Intelligent Key button can be selected as per the following in this mode.

- MODE 1: Press and hold
- MODE 2: Press twice
- MODE 3: Press and hold, or press twice

LO-BATT OF KEY FOB WARN | Intelligent Key low battery warning mode can be changed to operate (WITH) or not operate (WITHOUT) in this mode.
ANTI KEY LOCK IN FUNCTI | Key reminder function mode can be changed to operate (WITH) or not operate (WITHOUT) in this mode.
HAZARD ANSWER BACK | Hazard reminder function mode can be selected from the following in this mode.

- LOCK ONLY: Door lock operation only
- UNLOCK ONLY: Door unlock operation only
- LOCK/UNLOCK: Lock/unlock operation
- OFF: Non-operational

ANS BACK I-KEY LOCK | Buzzer reminder function (lock operation) mode by door request switch (driver side and passenger side) can be selected from the following is this mode.

- Horn chirp: Sound horn
- Buzzer: Sound Intelligent Key warning buzzer
- OFF: Non-operational

ANS BACK I-KEY UNLOCK | Buzzer reminder function (unlock operation) mode by door request switch can be changed to operate (ON) or not operate (OFF) in this mode.
SHORT CRANKING OUTPUT | Starter motor can operate during the times below.

- 70 msec
- 100 msec
- 200 msec

INSIDE ANT DIAGNOSIS | This function allows inside key antenna self-diagnosis.
HORN WITH KEYLESS LOCK | Horn reminder function mode by Intelligent Key button can be changed to operate (ON) or not operate (OFF) in this mode.

SELF-DIAG RESULT
Refer to DTC Index.
DATA MONITOR

Monitor Item | Condition
REQ SW -DR | Indicates [ON/OFF] condition of door request switch (driver side).
REQ SW -AS | Indicates [ON/OFF] condition of door request switch (passenger side).
REQ SW -BD/TR | Indicates [ON/OFF] condition of trunk opener request switch.
PUSH SW | Indicates [ON/OFF] condition of push-button ignition switch.
IGN RLY2 -F/B | Indicates [ON/OFF] condition of ignition relay 2.
ACC RLY-FB | NOTE： This item is displayed, but cannot be monitored.
CLUTCH SW | NOTE： This item is displayed, but cannot be monitored.
BRAKE SW 1 | Indicates [ON/OFF]* condition of brake switch power supply.
BRAKE SW 2 | Indicates [ON/OFF] condition of brake switch.
DETE/CANCL SW | Indicates [ON/OFF] condition of P position.
SFT PN/N SW | Indicates [ON/OFF] condition of P or N position.
S/L -LOCK | Indicates [ON/OFF] condition of steering lock unit (LOCK).
S/L -UNLOCK | Indicates [ON/OFF] condition of steering lock unit (UNLOCK).
S/L RELAY -F/B | Indicates [ON/OFF] condition of steering lock relay.
UNLK SEN -DR | Indicates [ON/OFF] condition of driver door UNLOCK status.
PUSH SW -IPDM | Indicates [ON/OFF] condition of push-button ignition switch.
IGN RLY1 -F/B | Indicates [ON/OFF] condition of ignition relay 1.
DETE SW -IPDM | Indicates [ON/OFF] condition of P position.
SFT PN -IPDM | Indicates [ON/OFF] condition of P or N position.
SFT P -MET | Indicates [ON/OFF] condition of P position.
SFT N -MET | Indicates [ON/OFF] condition of N position.
ENGINE STATE | Indicates [STOP/STALL/CRANK/RUN] condition of engine states.
S/L LOCK-IPDM | Indicates [ON/OFF] condition of steering lock unit (LOCK).
S/L UNLK-IPDM | Indicates [ON/OFF] condition of steering lock unit (UNLOCK).
S/L RELAY-REQ | Indicates [ON/OFF] condition of steering lock relay.
VEH SPEED 1 | Display the vehicle speed signal received from combination meter by numerical value [Km/h].
VEH SPEED 2 | Display the vehicle speed signal received from ABS or VDC or TCM by numerical value [Km/h].
DOOR STAT-DR | Indicates [LOCK/READY/UNLOCK] condition of driver side door status.
DOOR STAT-AS | Indicates [LOCK/READY/UNLOCK] condition of passenger side door status.
ID OK FLAG | Indicates [SET/RESET] condition of key ID.
PRMT ENG STRT | Indicates [SET/RESET] condition of engine start possibility.
PRMT RKE STRT | NOTE： This item is displayed, but cannot be monitored.
KEY SW -SLOT | Indicates [ON/OFF] condition of key slot.
TRNK/HAT MNTR | Indicates [ON/OFF] condition of trunk lid.
RKE-LOCK | Indicates [ON/OFF] condition of LOCK signal from Intelligent Key.
RKE-UNLOCK | Indicates [ON/OFF] condition of UNLOCK signal from Intelligent Key.
RKE-TR/BD | Indicates [ON/OFF] condition of TRUNK OPEN signal from Intelligent Key.
RKE-PANIC | Indicates [ON/OFF] condition of PANIC button of Intelligent Key.
RKE-P/W OPEN | NOTE： This item is displayed, but cannot be monitored.
RKE-MODE CHG | Indicates [ON/OFF] condition of MODE CHANGE signal from Intelligent Key.
RKE OPE COUN1 | When remote keyless entry receiver receives the signal transmitted while operating on Intelligent Key, the numerical value start changing.
RKE OPE COUN2 | NOTE： This item is displayed, but cannot be monitored.
REVERSE SWITCH | NOTE： This item is displayed, but cannot be monitored.
*: OFF is displayed when brake pedal is depressed while brake switch power supply is OFF.

ACTIVE TEST

Test item | Description
BATTERY SAVER | This test is able to check interior room lamp operation. The interior room lamp will be activated when “ON” on CONSULT-III screen is touched.
PW REMOTO DOWN SET | NOTE： This item is displayed, but cannot be used.
OUTSIDE BUZZER | This test is able to check Intelligent Key warning buzzer operation. The Intelligent Key warning buzzer will be activated when “ON” on CONSULT-III screen is touched.
INSIDE BUZZER | This test is able to check warning chime in combination meter operation.

- Take away warning chime sounds when “TAKE OUT” on CONSULT-III screen is touched.
- Key warning chime sounds when “KEY” on CONSULT-III screen is touched.
- P position warning chime sounds when “KNOB” on CONSULT-III screen is touched.

INDICATOR | This test is able to check warning lamp operation.

- “KEY” Warning lamp illuminates when “KEY ON” on CONSULT-III screen is touched.
- “KEY” Warning lamp blinks when “KEY IND” on CONSULT-III screen is touched.

INT LAMP | This test is able to check interior room lamp operation. The interior room lamp will be activated when “ON” on CONSULT-III screen is touched.
LCD | This test is able to check meter display information

- Engine start information displays when “BP N” on CONSULT-III screen is touched.
- Engine start information displays when “BP I” on CONSULT-III screen is touched.
- Key ID warning displays when “ID NG” on CONSULT-III screen is touched.
- Steering lock information displays when “ROTAT” on CONSULT-III screen is touched.
- P position warning displays when “SFT P” on CONSULT-III screen is touched.
- Intelligent Key insert information displays when “INSRT” on CONSULT-III screen is touched.
- Intelligent Key low battery warning displays when “BATT” on CONSULT-III screen is touched.
- Take away warning displays when “OUTKEY” on CONSULT-III screen is touched.
- OFF position warning displays when “LK WN” on CONSULT-III screen is touched.

TRUNK/GLASS HATCH | This test is able to check trunk lid opener actuator open operation. This actuator opens when “OPEN” on CONSULT-III screen is touched.
FLASHER | This test is able to check security hazard lamp operation. The hazard lamps will be activated when “RH” or “LH”on CONSULT-III screen is touched.
HORN | This test is able to check horn operation. The horn will be activated when “ON” on CONSULT-III screen is touched.
P RANGE | This test is able to check control device power supply Control device power is supplied when “ON” on CONSULT-III screen is touched.
ENGINE SW ILLUMI | This test is able to check push-ignition switch illumination operation. Push-ignition switch illumination illuminates when “ON” on CONSULT-III screen is touched.
LOCK INDICATOR | This test is able to check LOCK indicator in push-ignition switch operation. LOCK indicator in push-ignition switch illuminates when “ON” on CONSULT-III screen is touched.
ACC INDICATOR | This test is able to check ACC indicator in push-ignition switch operation. ACC indicator in push-ignition switch illuminates when “ON” on CONSULT-III screen is touched.
IGNITION ON IND | This test is able to check ON indicator in push-ignition switch operation. ON indicator in push-ignition switch illuminates when “ON” on CONSULT-III screen is touched.
KEY SLOT ILLUMI | This test is able to check key slot illumination operation. Key slot illumination illuminates when “ON” on CONSULT-III screen is touched.
TRUNK/BACK DOOR | This test is able to check trunk lid opener actuator open operation. This actuator opens when “OPEN” on CONSULT-III screen is touched.