1.CHECK AWD SOLENOID

1. Turn the ignition switch OFF.
2. Disconnect AWD solenoid harness connector.
3. Check the resistance between AWD solenoid harness connector terminals.

   AWD solenoid | Resistance (Approx.)
   Terminal
   1 | 2 | 1.75Ω

Is the inspection result normal?
YES>>INSPECTION END
NO>>AWD solenoid is malfunctioning. Replace electric controlled coupling. Refer to Exploded View (GT-R certified NISSAN dealer).