Item | Function
BCM | Controls the trunk open function.
Trunk lid opener actuator | Transmits trunk open operation to BCM.
Combination meter | Transmits vehicle seep signal to CAN communication line.
Remote keyless entry receiver | Receives lock/unlock signal from the Intelligent Key, and then transmits to BCM.
Trunk lid opener request switch | Inputs lock/unlock operation to BCM.
Intelligent Key | Transmits button operation to remote keyless entry receiver.
Outside key antenna (rear bumper) | Detects if Intelligent Key is outside the vehicle.
Inside key antenna (trunk room) | Detects if Intelligent Key is inside the vehicle.
Trunk lid opener cancel switch | Cancels the trunk open operation.
Intelligent Key warning buzzer | Warns the user of the open condition and inappropriate operations with the buzzer sound.
Trunk room lamp switch | Input trunk lid open/close condition to BCM.
Push-button ignition switch | Inputs push-button ignition switch ON/OFF condition to BCM.