1.PERFORM INITIALIZATION PROCEDURE Perform initialization of power window that is malfunctioning, and check that auto operation operates normally. Refer to Special Repair Requirement. Is the inspection result normal? YES>>INSPECTION END
NO>>GO TO 2.
2.CHECK POWER WINDOW AUTO CIRCUIT (POWER WINDOW SUB-SWITCH)
Check power window auto circuit (power window sub-switch).
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CONFIRM THE OPERATION
Confirm the operation again.
Is the inspection result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.