DTC DETECTION LOGIC NOTE： If DTC B2108 is displayed with DTC U1000, first perform the trouble diagnosis for DTC U1000. Refer to DTC Logic.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B2108 | STRG LCK RELAY ON | IPDM E/R detects that the relay is stuck in the ON position for about 1 second even if the IPDM E/R receives steering lock relay ON/OFF signal from BCM. | IPDM E/R

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Press the push-button ignition switch under the following conditions and wait for at least 1 second.

- Shift lever is in the P or N position.
- Do not depress brake pedal.

2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END