1.CHECK CONNECTOR

1. Turn the ignition switch OFF.
2. Disconnect the battery cable from the negative terminal.
3. Check the terminals and connectors of the combination meter for damage, bend and loose connection (unit side and connector side).

Is the inspection result normal?
YES>>GO TO 2.
NO>>Repair the terminal and connector.
2.CHECK HARNESS FOR OPEN CIRCUIT

1. Disconnect the connector of combination meter.
2. Check the resistance between the combination meter harness connector terminals.

   Combination meter harness connector | Resistance (Ω)
   Connector No. | Terminal No.
   M53 | 21 | 22 | Approx. 54 – 66

Is the measurement value within the specification?
YES>>GO TO 3.
NO>>Repair the combination meter branch line.
3.CHECK POWER SUPPLY AND GROUND CIRCUIT
Check the power supply and the ground circuit of the combination meter. Refer to Diagnosis Procedure.
Is the inspection result normal?
YES (Present error)>>Replace the combination meter. Refer to Exploded View.
YES (Past error)>>Error was detected in the combination meter branch line.
NO>>Repair the power supply and the ground circuit.