DTC DETECTION LOGIC Freeze frame data is not stored in the ECM for this self-diagnosis.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
P1211 | TCS control unit | ECM receives malfunction information from “ABS actuator and electric unit (control unit)”. |

- ABS actuator and electric unit (control unit)
- TCS related parts

DTC CONFIRMATION PROCEDURE
1.PRECONDITIONING
TESTING CONDITION:
Before performing the following procedure, confirm that battery voltage is more than 10.5 V at idle.
>> GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE

1. Start engine and let it idle for at least 60 seconds.
2. Check 1st trip DTC.

Is 1st trip DTC detected?
YES>>Diagnosis Procedure (GT-R certified NISSAN dealer)
NO>>INSPECTION END