REMOVAL

1.Remove tire with power tool. Refer to Exploded View.

2.Remove brake hose bracket. Refer to Exploded View.

3.Remove caliper assembly mounting bolts. Hang caliper assembly in a place where it will not interfere with work. Refer to Exploded View (GT-R certified NISSAN dealer).

4.Remove disc rotor. Refer to Removal and Installation (GT-R certified NISSAN dealer).

5.Set suitable jack under axle assembly.

6.Separate shock absorber from axle housing. Refer to Exploded View.

7.Remove cotter pin of suspension arm ball joint, and loosen nut. Refer to Exploded View.

8.Remove suspension arm mounting bolts and nuts from rear suspension member.

9.Remove suspension arm from axle housing. Refer to Exploded View.

10.Remove suspension arm.

INSTALLATION
Note the following and, install in the reverse order of removal.

- Perform final tightening of bolts and nuts at the vehicle installation position (rubber bussing), under unladen conditions with tires on level ground.
- Never reuse cotter pin.