INSPECTION AFTER INSTALLATION Check on Fuel Leakage

1.Turn ignition switch “ON” (with the engine stopped). With fuel pressure applied to fuel piping, check there are no fuel leakage at connection points.
NOTE：
Use mirrors for checking at points out of clear sight.

2.Start the engine. With engine speed increased, check again that there are no fuel leakage at connection points.
■ CAUTION ■
Never touch the engine immediately after stopped, as the engine becomes extremely hot.