■ CAUTION ■ IPDM E/R integrated relays are not serviceable parts, and must not be removed from the unit. REMOVAL

1.Remove the battery. Refer to Exploded View.

2.Remove the cowl top cover (RH). Refer to Exploded View.

3.Pull up the IPDM E/R assembly while pressing the pawls (A) on the back of the IPDM E/R cover B (1).

4.Remove the IPDM E/R cover A (1) while pressing the pawls (A) at the lower end of the IPDM E/R cover A.

5.Disconnect the harness connector. And then remove the IPDM E/R (1).

6.Remove the nuts (A). And then remove the bracket (1) from the vehicle.

INSTALLATION
Install in the reverse order of removal.