REMOVAL

1.Remove tires with power tool. Refer to Exploded View.

2.Remove rear diffuser. Refer to Exploded View.

3.Remove front lower link.
■ CAUTION ■
Apply a matching mark to the installation position for adjusting bolt and rear suspension member.

INSTALLATION
Note the following, and install in the reverse order of removal.

- Perform final tightening of bolts and nuts at the vehicle installation position (rubber bushing) under unladen condition with tires on level ground.