1.CHECK “AUTO LOCK SET” SETTING IN “WORK SUPPORT” Check “AUTO LOCK SET” setting in “WORK SUPPORT”. Refer to CONSULT-III Function (BCM - INTELLIGENT KEY). Is the inspection result normal? YES>>GO TO 2.
NO>>Set “AUTO LOCK SET” setting in “WORK SUPPORT”.
2.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.