1.PERFORM INITIALIZATION Perform initialization with CONSULT-III. For initialization, refer to “CONSULT-III Operation Manual NATS-IVIS/NVIS”. Does steering lock operate? YES>>INSPECTION END
NO>>GO TO 2.
2.REPLACE STEERING LOCK UNIT

1. Replace steering lock unit.
2. Perform initialization with CONSULT-III. For initialization, refer to “CONSULT-III Operation Manual NATS-IVIS/NVIS”.

Does steering lock operate?
YES>>INSPECTION END
NO>>GO TO 3.
3.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END