1.CHECK FRONT WIPER HI OPERATION IPDM E/R AUTO ACTIVE TEST

1. Start IPDM E/R auto active test. Refer to Diagnosis Description.
2. Check that the front wiper operates at the HI operation.

CONSULT-III ACTIVE TEST

1. Select “FRONT WIPER” of IPDM E/R active test item.
2. With operating the test item, check front wiper operation.

   Hi | : Front wiper (HI) operation
   Off | : Stop the front wiper.

Is front wiper (HI) operation normally?
YES>>Front wiper motor HI circuit is normal.
NO>>Refer to Diagnosis Procedure.