BCM CONSULT-III FUNCTION CONSULT-III performs the following functions via CAN communication with BCM.

Diagnosis mode | Function Description
DATA MONITOR | The BCM input/output signals are displayed.
ACTIVE TEST | The signals used to activate each device are forcibly supplied from BCM.

DATA MONITOR

Monitor Item | Contents
PUSH SW | Indicates [ON/OFF] condition of push switch.
UNLK SEN -DR | Indicates [ON/OFF] condition of unlock sensor.
VEH SPEED 1 | Indicates [Km/h] condition of vehicle speed signal from combination meter.
KEY CYL SW-TR | NOTE： This item is displayed, but cannot be monitored.
TR CANCEL SW | Indicates [ON/OFF] condition of trunk lid opener cancel switch.
TR/BD OPEN SW | Indicates [ON/OFF] condition of trunk lid opener switch.
TRNK/HAT MNTR | Indicates [ON/OFF] condition of trunk room lamp switch.
RKE-TR/BD | Indicates [ON/OFF] condition of trunk open signal from Intelligent Key remote controller button.

ACTIVE TEST

Test item | Description
TRUNK/GLASS HATCH | This test is able to check trunk lid opener actuator open operation. This actuator opens when “OPEN” on CONSULT-III screen is touched.