DESCRIPTION If the temperature felt by the customer is different than the air flow temperature controlled by the temperature setting, the A/C auto amp. control temperature can be adjusted to compensate for the temperature setting. HOW TO SET With CONSULT-III
Perform “TEMP SET CORRECT” of HVAC work support item.

Work support items | Display (°F) | Display (°C)
TEMP SET CORRECT | 6 | 3.0
5 | 2.5
4 | 2.0
3 | 1.5
2 | 1.0
1 | 0.5
0 (initial status) | 0 (initial status)
−1 | −0.5
−2 | −1.0
−3 | −1.5
−4 | −2.0
−5 | −2.5
−6 | −3.0

NOTE：

- When −3.0°C (−6°F) is corrected on the temperature setting set as 25.0°C (77°F), the temperature controlled by A/C auto amp. is 25.0°C (77°F) − 3.0°C (−6°F) = 22.0°C (72°F) and the temperature becomes lower than the temperature setting.
- When the battery cable is disconnected from the negative terminal or when the battery voltage becomes 10 V or less, the setting of the difference between the set temperature and control temperature may be cancelled.