1.CHECK ASCD INDICATOR FUNCTION Check ASCD indicator under the following conditions.

ASCD INDICATOR | CONDITION | SPECIFICATION
CRUISE LAMP |

- Ignition switch: ON

- MAIN switch: Pressed at the 1st time →
  at the 2nd time

ON → OFF
SET LAMP |

- MAIN switch: ON
- When vehicle speed is between 40 km/h (25 MPH) and 250 km/h (155 MPH)

- ASCD: Operating

ON

- ASCD: Not operating

OFF

Is the inspection result normal?
YES>>INSPECTION END
NO>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).