REMOVAL

1.Remove instrument lower panel RH. Refer to Exploded View.

2.Remove front floor spacer RH. Refer to Exploded View.

3.Disconnect E-SUS control unit connector. Refer to Exploded View (GT-R certified NISSAN dealer).

4.Remove mounting nuts (A).

5.Disconnect connectors, and then remove ECM (1) with bracket attached.

6.Remove power steering control unit. Refer to Exploded View (GT-R certified NISSAN dealer).

7.Disconnect intake door motor connector (A).

8.Disconnect the blower motor connector (B).

9.Remove mounting bolt (C) and screw (D), from blower unit (1).

10.Remove blower unit.
■ CAUTION ■
Move blower unit rightward, and remove locating pin (1 part) and joint. Then remove blower unit downward.

INSTALLATION
Installation is basically the reverse order of removal.
■ CAUTION ■
Make sure locating pin (A) and joint (B) are securely inserted.

| : Vehicle front