DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B1137 | SIDE MODULE LH [SHORT] | Front LH side air bag module circuit are shorted to each other |

- Disconnection of wiring harness and short
- Malfunction in front LH side air bag module
- Malfunction in air bag diagnosis sensor unit

DTC CONFIRMATION PROCEDURE
1.CHECK SELF-DIAG RESULT
With CONSULT-III

1. Turn ignition switch ON.
2. Perform “AIR BAG” Self Diagnostic Result.

Without CONSULT-III

1. Turn ignition switch ON.
2. Check the air bag warning lamp status. Refer to Air Bag Warning Lamp Diagnosis.

NOTE：
SRS does not enter diagnosis mode if no malfunction is detected in user mode.
Is malfunctioning part detected?
YES>>Refer to Diagnosis Procedure.
NO>>INSPECTION END