1.CHECK COOLING FAN RELAY

1. Turn ignition switch OFF.
2. Remove cooling fan relay.
3. Check the continuity between cooling fan relay terminals under the following conditions.

   Terminals | Conditions | Continuity
   3 and 5 | 12 V direct current supply between terminals 1 and 2 | Existed
   No current supply | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace cooling fan relay.