1.CHECK ASCD STEERING SWITCH

1. Turn ignition switch OFF.
2. Disconnect combination switch (spiral cable) harness connector.
3. Check resistance between combination switch (spiral cable) harness connector terminals under the following conditions.

   Combination switch (spiral cable) | Condition | Resistance (Ω)
   Connector | Terminals
   M303 | 13 and 16 | MAIN switch: Pressed | Approx. 0
   CANCEL switch: Pressed | Approx. 250
   SET/COAST switch: Pressed | Approx. 660
   RESUME/ACCELERATE switch: Pressed | Approx. 1,500
   All ASCD steering switches: Released | Approx. 4,000

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace ASCD steering switch