DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC Detection Condition | Possible causes
P2833 | Shift fork "A" position circuit low | A DTC is set if the 6th-Neutral position sensor voltage value received by TCM is less than 300 mV. |

- 6th-Neutral position sensor
- TCM
- Harness or connector
  (Open or short in the 6th-Neutral position sensor circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Turn ignition switch ON, and wait for 5 seconds or more.
2. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Turn ignition switch ON, and wait for 5 seconds or more.
2. Check self-diagnosis.

Is DTC P2833 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.