When doing work that applies to the list below, make sure to calibrate decel G sensor before running vehicle.

×: Required –: Not required
Situation | Calibration of decel G sensor
Removing/Installing ABS actuator and electric unit (control unit) | ×
Replacing ABS actuator and electric unit (control unit) | ×
Removing/Installing steering components | —
Replacing steering components | —
Removing/Installing suspension components | —
Replacing suspension components | —
Changing old tires to new ones | —
Adjusting wheel alignment | —
Removing/Installing yaw rate/side/decel G sensor | ×
Replacing yaw rate/side/decel G sensor | ×