CONSULT‐III DATA MONITOR REFERENCE VALUES

Monitor item | Measuring condition | Standard/Status
SPEED METER [km/h] | Ignition switch ON | While driving | Equivalent to speedometer reading NOTE： 655.35 is displayed when the malfunction signal is received
SPEED OUTPUT [km/h] | Ignition switch ON | While driving | Equivalent to speedometer reading NOTE： 655.35 is displayed when the malfunction signal is received
ODO OUTPUT [km] | Ignition switch ON | — | Equivalent to odometer reading in combination meter
TACHO METER [rpm] | Ignition switch ON | While driving | Approximately the same as tachometer reading NOTE： 8191.875 is displayed when the malfunction signal is received
FUEL METER [L] | Ignition switch ON | — | Values according to fuel level
W TEMP METER [°C] | Ignition switch ON | — | Values according to engine coolant temperature NOTE： 215 is displayed when the malfunction signal is input
ABS W/L | Ignition switch ON | ABS warning lamp ON | On
ABS warning lamp OFF | Off
VDC/TCS IND | Ignition switch ON | VDC OFF indicator lamp ON | On
VDC OFF indicator lamp OFF | Off
SLIP IND | Ignition switch ON | SLIP Indicator lamp ON | On
SLIP indicator lamp OFF | Off
BRAKE W/L | Ignition switch ON | Brake warning lamp ON | On
Brake warning lamp OFF | Off
DOOR W/L | Ignition switch ON |

- Door open warning display
- Trunk open warning display

On

- Door open warning is not displayed
- Trunk open warning is not displayed

Off
HI-BEAM IND | Ignition switch ON | High beam indicator lamp ON | On
High beam indicator lamp OFF | Off
TURN IND | Ignition switch ON | Turn signal indicator lamp ON | On
Turn signal indicator lamp OFF | Off
RR FOG IND | Ignition switch ON | This item is displayed, but cannot be monitored. | Off
OIL W/L | Ignition switch ON | Oil pressure warning lamp ON | On
Oil pressure warning lamp OFF | Off
LIGHT IND | Ignition switch ON | Tail lamp indicator lamp ON | On
Tail lamp indicator lamp OFF | Off
MIL | Ignition switch ON | Malfunction indicator lamp (MIL) ON | On
Malfunction indicator lamp (MIL) OFF | Off
CRUISE IND | Ignition switch ON | CRUISE indicator lamp ON | On
CRUISE indicator lamp OFF | Off
SET IND | Ignition switch ON | SET indicator lamp ON | On
SET indicator lamp OFF | Off
ATC/T‐AMT W/L | Ignition switch ON | Transmission warning lamp ON | On
Transmission warning lamp OFF | Off
4WD W/L | Ignition switch ON | AWD warning lamp ON | On
AWD warning lamp OFF | Off
FUEL W/L | Ignition switch ON | Low fuel warning display | On
Low fuel warning is not displayed | Off
WASHER W/L | Ignition switch ON | Low washer fluid warning display | On
Low washer fluid warning is not displayed | Off
AIR PRES W/L | Ignition switch ON | Tire pressure warning lamp ON | On
Tire pressure warning lamp OFF | Off
KEY G/Y W/L | Ignition switch ON | KEY warning lamp (green/yellow) ON | On
KEY warning lamp (green/yellow) OFF | Off
LCD | Ignition switch ON | Engine start indication is displayed | B&P I
Ignition switch ACC | Engine start indication is displayed | B&P N
Ignition switch LOCK | Key ID NG warning is displayed | ID NG
Ignition switch LOCK | Steering lock rotation operation signal illuminated | ROTAT
Ignition switch LOCK | P engagement warning is displayed | SFT P
Ignition switch LOCK | Key insertion indication is displayed | INSRT
Ignition switch LOCK | Intelligent Key low battery notice warning is displayed | BATT
Ignition switch ON | Key removal warning is displayed | NO KY
Ignition switch LOCK | Key reminder warning is displayed | OUT KY
Ignition switch ON | ACC warning is displayed | LK WN
SHIFT IND | Ignition switch ON | Shift position P is displayed | P
Shift position R is displayed | R
Shift position N is displayed | N
Shift position A1 is displayed | A1
Shift position A2 is displayed | A2
Shift position A3 is displayed | A3
Shift position A4 is displayed | A4
Shift position A5 is displayed | A5
Shift position A6 is displayed | A6
Shift position M1 is displayed | M1
Shift position M2 is displayed | M2
Shift position M3 is displayed | M3
Shift position M4 is displayed | M4
Shift position M5 is displayed | M5
Shift position M6 is displayed | M6
PKB SW | Ignition switch ON | Parking brake switch ON | On
Parking brake switch OFF | Off
BUCKLE SW | Ignition switch ON | Seat belt not fastened | On
Seat belt fastened | Off
BRAKE OIL SW | Ignition switch ON | Brake fluid level switch ON | On
Brake fluid level switch OFF | Off
A/C AMP CONN | Ignition switch ON | A/C auto amp. is not connected | On
A/C auto amp. is connected | Off
ENTER SW | Ignition switch ON | Enter switch is being pressed | On
Enter switch is not pressed | Off
SELECT SW | Ignition switch ON | Select switch is being pressed | On
Select switch is not pressed | Off
DISTANCE [km] | Ignition switch ON | — | Possible driving distance calculated by combination meter
OUTSIDE TEMP [°C] | Ignition switch ON | — | Equivalent to ambient air temperature NOTE： This may not match the indicated value on information display.
FUEL LOW SIG | Ignition switch ON | Low fuel warning is displayed | On
Low fuel warning is not displayed | Off
CRANKING SIG | At engine cranking | On
Ignition switch ON | Off
ST CNT SIG | At engine cranking | On
Ignition switch ON | Off
BUZZER | Ignition switch ON | Buzzer ON | On
Buzzer OFF | Off
ENG OIL TMP | Ignition switch ON | — | Values according to engine oil temperature
ENG OIL PRESS | Ignition switch ON | — | Values according to engine oil pressure
TM OIL TMP | Ignition switch ON | — | Values according to transmission oil temperature
TM OIL PRESS | Ignition switch ON | — | Values according to transmission oil pressure
A/F RATIO | Ignition switch ON | — | Values according to engine air-fuel ratio
BOOST PRESS | Ignition switch ON | — | Values according to boost pressure
THRTL POSI | Ignition switch ON | — | Values according to throttle position
TRQ DSTRBT | Ignition switch ON | — | Values according to front torque distribution rate
AMT P SFT | Ignition switch ON | Shift “ P ” warning display ON | On
Shift “ P ” warning display OFF | Off
AMT SYS CHCK | Ignition switch ON | Transmission system check display ON | On
Transmission system check display ON | Off
AMT SFT POSI | Ignition switch ON | Shift lever position warning display ON | On
Shift lever position warning display OFF | Off
AMT OIL TMP H | Ignition switch ON | Transmission oil high temperature warning display ON | On
Transmission oil high temperature warning display OFF | Off
AMT CL TMP H | Ignition switch ON | Transmission clutch high temperature warning display ON | On
Transmission clutch high temperature warning display OFF | Off
AMT CHCK | Ignition switch ON | It is displayed, but not used. | Off
AMT MALF | Ignition switch ON | Transmission system warning display ON | On
Transmission system warning display OFF | Off
TPMS FLT TIRE | Ignition switch ON | Run-flat tire warning display ON | On
Run-flat tire warning display OFF | Off
TPMS PRESS L | Ignition switch ON | Low tire pressure warning display ON | On
Low tire pressure warning display OFF | Off
TPMS MALF | Ignition switch ON | Tire pressure monitoring system warning display ON | On
Tire pressure monitoring system warning display OFF | Off
4WD CL TMP H | Ignition switch ON | AWD clutch high temperature warning display ON | On
AWD clutch high temperature warning display OFF | Off
4WD TIRE CHCK | Ignition switch ON | Front/rear tire size discrepancy warning display ON | On
Front/rear tire size discrepancy warning display OFF | Off
4WD SYS MALF | Ignition switch ON | AWD system warning display ON | On
AWD system warning display OFF | Off
ABS MALF | Ignition switch ON | Anti-lock braking system (ABS) warning display ON | On
Anti-lock braking system (ABS) warning display OFF | Off
VDC MALF | Ignition switch ON | Vehicle dynamic control (VDC) system warning display ON | On
Vehicle dynamic control (VDC) system warning display OFF | Off
ENG SYS CHCK | Ignition switch ON | Engine system warning display ON | On
Engine system warning display OFF | Off
ASCD SYS MALF | Ignition switch ON | CRUISE control system warning display ON | On
CRUISE control system warning display OFF | Off
ASCD REQ SPD | Ignition switch ON | While driving | Same value as ASCD set vehicle speed
ASCD STATUS | Ignition switch ON | ASCD system OFF | Off
ASCD system ON | ASCD
ASCD SPD BLNK | Ignition switch ON | Blinking status of ASCD set vehicle speed (displayed) | On
Blinking status of ASCD set vehicle speed (not displayed) | Off
NOTE：
Some items are not available according to vehicle specifications.

TERMINAL LAYOUT
INPUT/OUTPUT SIGNAL STANDARD

Terminal No. (Wire color) | Description | Condition | Value (Approx.)
+ | – | Signal name | Input/ Output
1 (V) | Ground | Battery power supply | Input | Ignition switch OFF | — | Battery voltage
2 (W) | Ground | Ignition power supply | Input | Ignition switch ON | — | Battery voltage
3 (B) | Ground | Ground | — | Ignition switch ON | — | 0 V
5 (B) | Ground | Ground | — | Ignition switch ON | — | 0 V
6 (W) | Ground | Meter control switch ground | — | Ignition switch ON | — | 0 V
7 (Y) | Ground | A/C auto amp. connection recognition signal | Input | Ignition switch ON | — | 5 V
8 (SB) | Ground | Ambient sensor ground | — | Ignition switch ON | — | 0 V
9 (P) | Ground | Ambient sensor | Input | Ignition switch ON | — | Refer to Component Inspection.
12 (L) | Ground | Vehicle speed signal (2-pulse) | Output | Ignition switch ON | Vehicle speed is approximately 40 km/h (25 MPH) | NOTE： The maximum voltage varies depending on the specification (destination unit).
13 (V) | Ground | Vehicle speed signal (8-pulse) | Output | Ignition switch ON | Vehicle speed is approximately 40 km/h (25 MPH) | NOTE： The maximum voltage varies depending on the specification (destination unit).
14 (B) | Ground | Oil pressure sensor ground | — | Ignition switch ON | — | 0 V
15 (R) | Ground | Air bag signal | Input | Ignition switch ON | Air bag warning lamp ON | 5 V
Air bag warning lamp OFF | 0 V
18 (L) | Ground | Fuel level sensor signal ground | — | Ignition switch ON | — | 0 V
19 (R) | Ground | Oil level sensor ground | — | Ignition switch ON | — | 0 V
20 (W) | Ground | Oil level sensor signal | Input | Ignition switch ON | — | Refer to Component Inspection.
21 (L) | Ground | CAN-H | — | Ignition switch ON | — | —
22 (P) | Ground | CAN-L | — | Ignition switch ON | — | —
23 (LG) | 6 (W) | Illumination control switch signal (–) | Input | Ignition switch ON | When switch is pressed | 0 V
Other than the above | 5 V
24 (BR) | 6 (W) | Illumination control switch signal (+) | Input | Ignition switch ON | When switch is pressed | 0 V
Other than the above | 5 V
25 (G) | 6 (W) | Trip A/B reset switch signal | Input | Ignition switch ON | When trip A/B reset switch is pressed | 0 V
Other than the above | 5 V
26 (O) | 6 (W) | Enter switch signal | Input | Ignition switch ON | When enter switch is pressed | 0 V
Other than the above | 5 V
27 (SB) | 6 (W) | Select switch signal | Input | Ignition switch ON | When select switch is pressed | 0 V
Other than the above | 5 V
28 (BR) | Ground | Alternator signal | Input | Ignition switch ON | Charging warning lamp ON | 0 V
Charging warning lamp OFF | 12 V
29 (G) | Ground | Seat belt buckle switch signal (passenger side) | Input | Ignition switch ON |

- When getting in the passenger seat
- When passenger seat belt is fastened.

12 V

- When getting in the passenger seat
- When passenger seat belt is unfastened

0 V
30 (LG) | Ground | Seat belt buckle switch signal (driver side) | Input | Ignition switch ON | When driver seat belt is fastened | 12 V
When driver seat belt is unfastened | 0 V
31 (V) | Ground | Parking brake switch signal | Input | Ignition switch ON | Parking brake applied | 0 V
Parking brake released | 5 V
32 (V) | Ground | Brake fluid level switch signal | Input | Ignition switch ON | Brake fluid level is normal | 0 V
Brake fluid level is MIN level or less | 5 V
33 (L) | Ground | Washer level switch signal | Input | Ignition switch ON | Low washer fluid warning display ON | 0 V
Low washer fluid warning display OFF | 5 V
34 (GR) | Ground | Oil pressure sensor power | Output | Ignition switch ON | — | 5 V
35 (W) | Ground | Oil pressure sensor signal | Input | Ignition switch ON | — | Refer to Component Inspection.
38 (O) | Ground | Fuel level sensor signal | Input | Ignition switch ON | — |