DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
C1210 | ENGINE SIGNAL 1 | Malfunction related to engine signal has been detected. | Malfunction of engine control system

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Start the engine. Drive the vehicle for a while.
2. Perform AWD control unit self-diagnosis for “ALL MODE AWD/4WD”.

Is DTC “C1210” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END