REMOVAL

1.Remove the engine assembly with the suspension member from the vehicle. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Remove the front final drive assembly from the engine assembly with power tool. Refer to Exploded View (GT-R certified NISSAN dealer).
■ CAUTION ■

- The left side oil seal is joined with the engine oil pan, therefore the final drive assembly must be removed from the engine assembly before replacing the oil seal.
- The engine oil pan (upper) uses heat-resistant magnesium. Never apply an impact to it.

3.Remove the side oil seal using a suitable tool.
■ CAUTION ■
Never damage gear carrier.

INSTALLATION

1.Apply multi-purpose grease to sealing lips of side oil seal.

2.Using the drift (A) [SST: KV38102100 (J-25803-01)], press-fit side oil seal so that its surface comes face‐to‐face with the end surface of the gear carrier.
■ CAUTION ■

- Never reuse oil seal.
- When installing, never incline oil seal.

3.Install the front final drive assembly on the engine assembly. Refer to Exploded View (GT-R certified NISSAN dealer).

4.Install the engine assembly with the suspension member on the vehicle. Refer to Exploded View (GT-R certified NISSAN dealer).

5.When oil leaks while removing, check oil level after the installation. Refer to Inspection.