1.CHECK TRANSMITTERS With CONSULT-III

1. Adjust the tire pressures to the specified value for all wheels. Refer to Tire.
2. Perform transmitter ID registration for all wheels. Refer to Transmitter ID Registration Procedure.
3. Within 15 minutes, use CONSULT-III “DATA MONITOR” to display the tire pressure for all wheels.
4. Check that “DATA MONITOR” displayed a tire pressure of 438.60 kPa (4.47kg/cm2, 63.60 psi).

   Monitor item | condition | Displayed value
   AIR PRESS FL | Drive for several minutes at a speed of 40 km/h (25 MPH) or more, then stop the vehicle. | Internal pressure of tires
   AIR PRESS FR
   AIR PRESS RR
   AIR PRESS RL

Is the inspection result normal?
YES>>Replace the malfunctioning transmitter.
NO>>INSPECTION END