Horn relay 2 1.CHECK HORN RELAY 2

1. Turn ignition switch OFF.
2. Disconnect horn relay 2.
3. Check horn relay 2.

Horn relay 2 | Condition | Voltage(V) (Approx.)
Terminal
3 | 12 V direct current supply between terminals 1 and 2. | 12V
No current supply | 0V

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace horn relay 2.
Diode
1.CHECK DIODE

1. Turn ignition switch OFF.
2. Disconnect diode.
3. Check the continuity between diode terminals under the following conditions..

Terminal | Continuity
(+)* | (-)*
1 | 2 | Existed
2 | 1 | Not existed
*: For a digital tester.

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace diode.