DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1D10 | F VERTICAL G-SEN |

- A malfunction occurs in the output voltage from the front vertical G sensor.
- A malfunction occurs in the supply voltage to the front vertical G sensor.

- Harness or connector
- Front vertical G sensor
- E-SUS control unit

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Turn the ignition switch OFF to ON.
2. Perform “E-SUS” self-diagnosis.

Is DTC “C1D10” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END