DETAILED FLOW 1.COLLECT THE INFORMATION FROM THE CUSTOMER It is also important to clarify customer complaints before inspection. First of all, reproduce symptoms and understand them fully. Ask customer about his/her complaints carefully. In some cases, it is necessary to check symptoms by driving vehicle with customer.
■ CAUTION ■
Customers are not professional. It is dangerous to make an easy guess like “maybe the customer means that...,” or “maybe the customer mentions this symptom”.
>>GO TO 2.
2.CHECK THE STATUS

1. Power steering fluid leakage and check the power steering fluid level. Refer to Inspection.
2. Check the drive belt tension. Refer to Checking.
3. Check the power steering gear for damages, cracks and fluid leakage. Refer to Inspection (GT-R certified NISSAN dealer).
4. Check the relief oil pressure. Refer to Inspection (GT-R certified NISSAN dealer).

>> GO TO 3.
3.DIAGNOSIS CHART BY SYMPTOM
Perform the diagnosis by symptom. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
>>GO TO 4.
4.FINAL CHECK
Check the input/output standard values for the power steering control unit.
Are the power steering control unit input/output values within standard ranges respectively?
YES>>INSPECTION END
NO>>GO TO 2.