DTC DETECTION LOGIC ■ CAUTION ■

- Before TCM is replaced, the IP characteristics must be extracted, based on the information read out from the malfunctioning TCM. For reading out the IP characteristic data, refer to “CONSULT-III GT-R TCM CONFIGURATION MANUAL”.
- If no IP characteristic data can be extracted TCM and the transmission assembly must be replaced as a set.

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P06B0 | Sensor power supply A circuit/open | DTC is set if malfunction is detected in power supply to sensor from TCM. | TCM

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE (PART 1)
With CONSULT-III

1. Start the engine.
2. Select “RANGE”, “GEAR” and “ENGINE SPEED” in “Data Monitor”.
3. Run the vehicle and maintain the following conditions for 5 seconds or more.

   RANGE | : M
   GEAR | : 4
   ENGINE SPEED | : 1,500 rpm or more

4. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine.
2. Run the vehicle and maintain the following conditions for 5 seconds or more.

   Shift lever | : M range
   Gear | : 4
   Engine speed | : 1,500 rpm or more

3. Check self-diagnosis.

Is DTC P06B0 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.