DISASSEMBLY

1.Place the glass mirror upward.

2.Put a strip of protective tape (B) on housing assembly.

3.As shown in the figure, insert a small flat-bladed screwdriver (A) between glass mirror (1) and actuator (2). Push up both pawls simultaneously to remove glass mirror lower half side.
NOTE：
Insert flat-bladed screwdriver, and push up while rotating (twisting) to make work easier.

4.Remove two terminals of mirror heater attachment.

5.Lightly lift up lower side of glass mirror, and detach both pawls of upper side as if pulling it out to disassemble glass mirror from actuator.

ASSEMBLY
Assemble in the reverse order of disassembly.
■ CAUTION ■
After installation, check that pawls are securely engaged.