1.PERFORM SELF-DIAGNOSIS With CONSULT-III

1. Erase self-diagnostic results for “ALL MODE AWD/4WD”.
2. Turn the ignition switch OFF, and then wait 10 seconds or more.
3. Perform self-diagnosis for “ALL MODE AWD/4WD”.

Is DTC “C1201” detected?
YES>>Replace AWD control unit. Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>Check AWD control unit pin terminals for damage or loose connection with harness connector. If any items are damaged, repair or replace damaged parts.