1.CHECK PARK POSITION SWITCH (PART 1) Check continuity between park position switch connector terminals.

Park position switch connector | Condition | Continuity
Connector | Terminal
B122 | 1 | 2 | Parking lever: P position. | Existed
Other than the above positions. | Not existed

Is the inspection result normal?
YES>>GO TO 2.
NO>>Repair or replace damaged parts.
2.CHECK PARK POSITION SWITCH (PART 2)
Check continuity between park position switch connector terminal and ground.

Park position switch connector | Ground | Continuity
Connector | Terminal
B122 | 1 | Ground | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Repair or replace damaged parts.