INSPECTION AFTER REMOVAL Lining Thickness Inspection Check thickness (A) of lining.

A | : Refer to Parking Drum Brake.

Drum Inner Diameter Inspection
Check inner diameter (B) of drum.

B | : Refer to Parking Drum Brake.

Other Inspections
Check the following items, and replace the parts if necessary.

- Lining for excessive wear, damage or peeling.
- Brake shoe sliding surface for excessive wear or damage.
- Anti-rattle pin and retainer for excessive wear, damage or rust.
- Adjuster spring, return spring and anti-rattle spring for settling, excessive wear, damage or rust.
- Adjuster for smoothness.
- Toggle lever for excessive wear, damage or rust.
- Visually check inside of the drum for excessive wear, cracks or damage with a pair of vernier calipers.

ADJUSTMENT AFTER INSTALLATION
Check the parking brake for drag. Perform the following procedure if necessary.

1.Adjust the parking brake lever stroke. Refer to Inspection and Adjustment.

2.Check the parking brake for drag again. Check the rear disc brake for drag if necessary. Refer to Inspection and Adjustment.