- The 3rd-5th position sensor is installed on the actuator control valve and detects the sleeve B2 position.
- The 3rd-5th position sensor converts the sleeve B2 position into output voltage and transmits the signal to TCM.
- The sleeve B2 has its oil passage secured by the shift solenoid valve 3 and shift solenoid valve 2 when the sequence solenoid valve is ON and is driven by the axis B feed pressure solenoid valve. The 3rd gear and 5th gear are selected or deselected depending on the operation of the sleeve B2.