- Always tighten each mounting bolt and nut to the specified torque when they are cold.
- When performing removal or installation work, check for any foreign materials entered. If any, eliminate or clean them.
- Check that the wheel hub and bearing assemblies have no backlash and no jerky motion in rotation direction. When changing engine oil, be sure to check them with the road wheels removed.
- Tighten up wheel hub lock nut within tightening torque of 250 N·m (26 kg-m, 184 ft-lb) before and after sports driving.