1.CHECK WASHER LEVEL SWITCH SIGNAL CIRCUIT Check the washer level switch signal circuit. Refer to Diagnosis Procedure. Is the inspection result normal? YES>>GO TO 2. NO>>Repair the harnesses or connectors.
2.CHECK WASHER LEVEL SWITCH COMPONENT PARTS
Perform the inspection of washer level switch component parts. Refer to Component Inspection.
Is the inspection result normal?
YES>>Replace the combination meter.
NO>>Replace the washer level switch. Refer to Removal and Installation.