REMOVAL

1.Lift up the vehicle.

2.Remove EVAP canister fixing bolt.

3.Remove EVAP canister.

NOTE：
The EVAP canister vent control valve and EVAP canister system pressure sensor can be removed without removing the EVAP canister.
INSTALLATION
Install in the reverse order of removal.
NOTE：
Tighten EVAP canister fixing bolt to the specified torque.
DISASSEMBLY

1.Turn EVAP canister vent control valve counterclockwise.

A | : Lock
B | : Unlock

2.Remove the EVAP canister vent control valve.

ASSEMBLY
Assemble in the reverse order of disassembly.
■ CAUTION ■
Always replace O-ring with a new one.