1.PERFORM INITIALIZATION PROCEDURE Perform initialization of power window that is malfunctioning, and check that automatic window adjusting function operates normally. Refer to Special Repair Requirement. Is the inspection result normal? YES>>INSPECTION END
NO>>GO TO 2.
2.CHECK DOOR SWITCH CIRCUIT
Check door switch circuit.
Refer to Component Function Check.
Is the inspection result normal?
YES>>Replace malfunctioning power window motor. Refer to Removal and Installation (GT-R certified NISSAN dealer).
NO>>Repair or replace the malfunctioning parts.