REMOVAL

1.Remove the body side welt (LH/RH) and the front pillar garnish (LH/RH). Refer to Removal and Installation.

2.Disconnect the inside mirror harness connector. Refer to Removal and Installation.

3.Disengage the clips (B) and then, disconnect the connector (A) of roof harness of front pillar LH.

4.Remove the sun-visor assembly (LH/RH).

- Remove the sun-visor cover (LH/RH).
- Remove the mounting screw (B) of sun-visor (1) (LH/RH) using screwdriver (A).
- Disconnect the vanity mirror lamp harness connector.

5.Rotate the sun-visor holder (1) 90 degrees counterclockwise, pull it downward, and then remove.

6.Remove the kicking plate inner (LH/RH), rear seat cushion back (LH/RH), rear side finisher (LH/RH), rear pillar finisher (LH/RH), and rear body side welt (LH/RH). Refer to Removal and Installation.

7.Remove the passenger side front seat. Refer to Removal and Installation.

8.Remove the control device. Refer to Removal and Installation.

9.Remove the center console assembly. Refer to Removal and Installation.

10.Remove the rear hidden clips from the roof panel at the rear end of the headlining, using a remover tool.

11.Disengage the joint of dual-lock fastener (A) and metal clip (B) of roof console assembly.

| : Metal clip

12.Check that the dual-lock fastener on the front end of the headlining is removed. If it is not removed, use a remover tool to remove it.
■ CAUTION ■

- Roof console assembly is crimped from the back of headlining. Remove it by disengaging the crimped area from back of roof console assembly after removing headlining from the vehicle.
- Never wrinkle the headlining by bending during work.

13.Remove the headlining from passenger side door opening.
■ CAUTION ■

- 2 workers are required for removal in order to prevent damage.
- Apply protective tape to the portion where contact may occur during work.
- Never bend headlining when removing.

14.Remove the following parts after removing the headlining.

- Remove roof console assembly.
- Map lamp assembly. Refer to Removal and Installation.
- Antenna feeder assembly. Refer to Feeder layout.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- First install the metal clip of map lamp and the clip of the rear end of the headlining for positioning.
- Never bend headlining when installing.